[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 3: A/C outlet air temperature cannot be set. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 3: A/C outlet air temperature cannot be set.
| COMMENTS ON TROUBLE SYMPTOM When the blower air temperature can not be changed even if the preset temperature is changed, the sensors, the air mixing door control motor and potentiometer or the A/C-ECU may be defective.
| POSSIBLE CAUSES Malfunction of the A/C-ECU
| DIAGNOSIS
| Read diagnosis code by using the MUT-II/III. Q: Is the diagnosis code set? YES: Refer to diagnosis code chart . NO: Replace the automatic air conditioner control panel (A/C-ECU).

[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 3: A/C outlet air temperature cannot be set. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation