[26] FRONT AXLE - - ON-VEHICLE SERVICE - HUB BOLT REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| HUB BOLT REPLACEMENT Remove the caliper assembly and suspend it with wire so that it does not fall. Remove the brake disc.
| Use the following special tools to remove the hub bolts. Front hub and flange yoke holder (MB990767) Hub bolt remover (MB991618)
| Install the plain washer to the new hub bolt, and install the bolt with a nut. Install the brake disc, caliper assembly and tighten the caliper assembly mounting bolts to the specified torque 100 ± 10 N·m.

[26] FRONT AXLE - - ON-VEHICLE SERVICE - HUB BOLT REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation