[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - DIAGNOSIS CODE CHART | PRINT PAGE / INDEX / PRIOR / NEXT

DIAGNOSIS CODE CHART
Code No. | Diagnosis Detail | Reference page
--- | --- | ---
11 | Trouble related to the ETACS-ECU |
12 | Trouble related to the column switch or improper connection to the ETACS-ECU |
13 | Trouble related to the front-ECU or improper connection to the ETACS-ECU |
21 | Short circuit in SWS communication line |
31 | Open circuit in the signal line between the SRS-ECU and the ETACS-ECU (impact detection signal) |
32 | Short circuit in the signal line between the SRS-ECU and the ETACS-ECU (impact detection signal)

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - DIAGNOSIS CODE CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation