[13D] FUEL SUPPLY - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
4G63 The fuel system consists of the following components: Fuel injector Fuel delivery pipe Fuel pressure regulator Fuel tank assembly Fuel vapour canister Fuel tank safety valve Fuel tank gauge unit Fuel pump assembly <2WD> Fuel tank pump and gauge assembly <4WD>
SPECIFICATIONS
ITEM | SPECIFICATION
--- | ---
Fuel tank capacity L | 60
Fuel pump type | Electric type
Fuel filter type | Cartridge (incorporator fuel pump module)
Fuel return system | Fuel pressure regulator return
Fuel pressure regulator control pressure kPa | 4G63 | 328
4G63-T/C | 294
Fuel injector | Type | Electromagnetic type
Quantity | 4
Evaporative emission control system | Canister type
4G64 The fuel system consists of the following components: Fuel injector Fuel delivery pipe Fuel pressure regulator Fuel tank assembly Fuel vapour canister Fuel tank safety valve Fuel tank gauge unit Fuel tank pump and gauge assembly
SPECIFICATIONS
ITEM | SPECIFICATION
--- | ---
Fuel tank capacity L | 60
Fuel pump type | Electric type
Fuel filter type | Cartridge (incorporator fuel pump module)
Fuel return system | Fuel pressure regulator return
Fuel pressure regulator control pressure kPa | 328
Fuel injector | Type | Electromagnetic type
Quantity | 4
Evaporative emission control system | Canister type
4G69
The fuel system consists of the following components: Fuel injector Fuel delivery pipe Fuel tank assembly Fuel vapour canister Fuel tank safety valve Fuel tank gauge unit Fuel tank pump and gauge assembly (incorporating fuel pump pressure regulator) Fuel tank levelling valve assembly <Vehicles for Brazil and Chile> Fuel tank temperature sensor <Vehicles for Brazil and Chile>
The fuel system of vehicles with 4G69 engine has the following characteristics. A plastic tube (a conductive multilayer nylon tube) is used for the fuel high-pressure hose in the engine compartment to improve fuel supply performance and reduce the weight. A returnless fuel system eliminates returned fuel from the engine. The heat that fuel receives from the engine is reduced, minimizing fuel temperature in the fuel tank and controlling the amount of evaporated gas.
SPECIFICATIONS
Item | Specification
--- | ---
Fuel tank capacity L | 60
Fuel pump type | Electric
Fuel filter type | Cartridge (incorporating fuel pump)
Fuel return system | Fuel pump pressure regulator return
Fuel pump pressure regulator control pressure kPa | 324
Fuel injector | Type | Electro-magnetic
Quantity | 4
Evaporative emission control system | Canister

[13D] FUEL SUPPLY - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation