[54A] CHASSIS ELECTRICAL - - DIAGNOSTIC SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

DIAGNOSTIC SYSTEM Service quality has been improved by fitting diagnosis connectors for the MUT-II/III inspection near the left <L.H. drive vehicles> and right <R.H. drive vehicles> knee area of the driver's seat on the instrument panel.
Diagnostic function | MPI | ABS | A/T | Immobilizer | SRS | ETACS
--- | --- | --- | --- | --- | --- | ---
Diagnosis code set | × | × | × | × | × | ×
Diagnosis code output by voltmeter | - | - | - | - | - | ×
Output of service data | × | × | × | - | × | -
Actuator test | × | × | × | - | - | -
Diagnostic output by warning lamp and indicator lamp | - | × (ABS warning lamp) | - | - | - | -
Diagnosis record storage | × | × | × | × | × | -
Erasure of diagnosis code by the MUT-II/III | × | × | × | × | × | -
Pulse check by MUT-II/III | - | - | - | - | - | ×
DIAGNOSIS CONNECTORS
Diagnosis connector (Black)
1 | Diagnosis control
2,3 | -
4 | Earth
5 | Earth
6 | -
7 | MPI, ABS, A/T, Immobilizer, SRS
8 | -
9 | ETACS-ECU
10 | -
11 | -
12 | -
13 | -
14 | Simulated vehicle speed signal
15 | -
16 | Battery
Diagnosis connector (White)
21 - 23 | -
24 | MPI
25 - 30 | -
31 | SWS communication line
32 | -
33 | -

[54A] CHASSIS ELECTRICAL - - DIAGNOSTIC SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation