[37] POWER STEERING - - STEERING GEAR | PRINT PAGE / INDEX / PRIOR / NEXT

STEERING GEAR Using the following parts have contributed to save weight; an aluminium steering gear and linkage valve housing, a plastic tie-rod bellows, and the hollow-type tie-rod stud. The installation accuracy, rigidity and steering stability have been improved by using an eye bushing, which secures the steering gear to the crossmember.

[37] POWER STEERING - - STEERING GEAR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation