[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D4. CHECK BRAKE PADS AND DISCS FOR WEAR | PRINT PAGE / INDEX / PRIOR / NEXT

| D4. CHECK BRAKE PADS AND DISCS FOR WEAR
| Check the brake pad thickness through the caliper body check port. Standard value: 10.0 mm Limit: 2.0 mm When the thickness is less than the limit, always replace the pads at an axle set.
| Using a micrometer, measure disc thickness at eight positions, approximately 45° apart and 10 mm in from the outer edge of the disc. Standard value: 26.0 mm <Front (1 piston type)> 24.0 mm <Front (2 piston type)> 10.0 mm <Rear> Limit: 24.4 mm <Front (1 piston type)> 22.4 mm <Front (2 piston type)> 8.4 mm <Rear> If the disk thickness is less than the limits, replace it with a new one.
| BRAKE DISC RUN-OUT CHECK Remove the brake assembly, and then hold it with wire. Temporarily install the disc with the hub nut.
| Place a dial gauge approximately 5 mm from the outer circumference of the brake disc, and measure the run-out of the disc. Limit: 0.04 mm <Front> 0.05 mm <Rear>

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D4. CHECK BRAKE PADS AND DISCS FOR WEAR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation