[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - WATER TEST | PRINT PAGE / INDEX / PRIOR / NEXT

| ON-VEHICLE SERVICE

| WATER TEST Check if there are any leaks in the sunroof by the following procedure. Fully close the roof lid glass. Adjust the water pressure so that water comes out of the hose to a height of approximately 50 cm when the hose is held vertically facing upwards.
| Hold the end of the hose approximately 30 cm above the roof and let the water run onto the weatherstrip for 5 minutes or more. Check if any water leaks can be found in the room while watering. Even though there are any water leaks around the roof lid glass, it can be acceptable as long as water is caught in the drip area.

[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - WATER TEST | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation