[11D] ENGINE OVERHAUL <4G6-DOHC> - - WATER PUMP AND WATER HOSE - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

WATER PUMP AND WATER HOSE

REMOVAL AND INSTALLATION
|  |  | Removal sequence
--- | --- | --- | ---
|  | 1. | Water hose
|  | 2. | Water hose
|  | 3. | Water hose
|  | 4. | Water hose
| >>E<< | 5. | Engine coolant temperature sensor
| >>D<< | 6. | Engine coolant temperature gauge unit
|  | 7. | Water inlet fitting
|  | 8. | Thermostat
| >>C<< | 9. | Water outlet fitting
| >>B<< | 10. | Thermostat housing
| >>A<< | 11. | O-ring
| >>A<< | 12. | Water inlet pipe
| >>A<< | 13. | O-ring
|  | 14. | Water pump
|  | 15. | Water pump gasket
| INSTALLATION SERVICE POINTS
| >>A<< O-RING/WATER INLET PIPE INSTALLATION CAUTION Never allow any oil or grease to touch the O-rings. Clamp the water inlet pipe only after installation of the thermostat case. Replace the O-rings at both ends of the water inlet pipe with new ones. Insert the O-rings into the water pump and thermostat housing after wetting their peripheries with water.
| >>B<< THERMOSTAT HOUSING INSTALLATION
| Remove all old FIPG remaining on the thermostat housing and cylinder head. Apply a 2.7 ± 0.3 mm diameter bead of FIPG on the indicated surface of the thermostat housing. Specified sealant: Mitsubishi Genuine Part No.MD970389 or equivalent
| >>C<< WATER OUTLET FITTING INSTALLATION
| Remove all old FIPG remaining on the water outlet fitting and thermostat housing. Apply a 2.7 ± 0.3 mm diameter bead of FIPG to the indicated surface of the water outlet fitting. Specified sealant: Mitsubishi Genuine Part No.MD970389 or equivalent
| >>D<< ENGINE COOLANT TEMPERATURE GAUGE UNIT INSTALLATION
| Remove all old sealant remaining on the threaded hole in the engine coolant temperature gauge unit and the thermostat housing. NOTE: A new engine coolant temperature gauge unit is coated with sealant. It does not require coating with sealant before installation. Apply sealant to the indicated threads of the engine coolant temperature gauge unit. Specified sealant: 3M Nut Locking Part No.4171 or equivalent
| >>E<< ENGINE COOLANT TEMPERATURE SENSOR INSTALLATION
| CAUTION When using a tool, avoid letting it touch the connector portion which is made of plastic. Remove all old sealant remaining on the threads of the engine coolant temperature sensor and in the threaded hole in the thermostat housing. Apply sealant to the engine coolant temperature sensor's threads indicated in the drawing. Specified sealant: 3M ATD Part No.8660 or equivalent

[11D] ENGINE OVERHAUL <4G6-DOHC> - - WATER PUMP AND WATER HOSE - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation