[55] HEATER, AIR CONDITIONER AND VENTILATION - - VENTILATION SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

VENTILATION SYSTEM
DESCRIPTION OF STRUCTURE AND OPERATION The adoption of the following mechanism has increased air volume for ventilation and has achieved a ventilation system for defogging windows. Adopting the flow-speed type defroster and the unified heater system improves the defroster capacity and speed. Optimizing areas of the outside air induction hole and the air outlet improves ventilated air amount consisting with the quietness of the room.

[55] HEATER, AIR CONDITIONER AND VENTILATION - - VENTILATION SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation