[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SEAT BELTS WITH PRE-TENSIONER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

SEAT BELTS WITH PRE-TENSIONER

REMOVAL AND INSTALLATION
WARNING Disconnect the negative battery terminal and wait for 60 seconds or more before starting work. Furthermore, the disconnected battery terminal should be covered with tape to insulate it. Never attempt to disassemble or repair the seat belt pre-tensioner. If faulty, replace it. Be extremely careful when handling the seat with pre-tensioner. Do not subject it to shocks, drop it, bring it close to strong magnets or allow contact with water, grease or oil. Always replace it with a new part if any dents, cracks or deformation is found. Do not place anything on top of the seat belt pre-tensioner. Do not expose the seat belt pre-tensioner to temperatures over 90°C. After operating the seat belt pre-tensioner, replace the seat belt pre-tensioner with a new part. Gloves and protective goggles should be worn when handling a seat belt pre-tensioner once it has been used. If disposing of a seat belt with pre-tensioner which has not yet been operated, its seat belt pre-tensioner should be operated first before disposal (Refer to ).
Pre-removal Operation Turn the ignition key to the "LOCK" (OFF) position. Disconnect the Negative Battery Terminal.
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Sash guide cover
|  | 2. | Seat belt shoulder anchor bolt
|  | 3. | Seat belt lower anchor bolt
|  | • | Centre pillar trim, lower (Refer to GROUP 52A - Trims ).
<<A>> |  | 4. | Pre-tensioner connector connection
|  | 5. | Bracket
|  | 6. | Seat belt with pre-tensioner
|  |  | Installation steps
| >>A<< | • | Pre-installation inspection
|  | 6. | Seat belt with pre-tensioner
|  | 5. | Bracket
| >>B<< | 4. | Pre-tensioner connector connection
|  | • | Centre pillar trim, lower (Refer to GROUP 52A - Trims ).
|  | 3. | Seat belt lower anchor bolt
|  | 2. | Seat belt shoulder anchor bolt
|  | 1. | Sash guide cover
|  | • | Negative battery cable connection
| >>C<< | • | Post-installation inspection
NOTE: The figure shows the seat belt with pre-tensioner (RH).
| REMOVAL SERVICE POINTS
| <<A>>PRE-TENSIONER CONNECTOR DISCONNECTION
| Use a flat-tipped screwdriver to pull out forward and unlock the locking button of the harness-side connector. Disconnect the pretensioner connector.
| INSTALLATION SERVICE POINTS
| >>A<< PRE-INSTALLATION INSPECTION WARNING When discarding the seat belt with pre-tensioner, operate the pre-tensioner as specified in the service procedure (Refer to ). Even new seat belt with pre-tensioner require inspection before installation. Connect the negative battery cable. CAUTION Turn the ignition switch to the "LOCK" (OFF) position when connecting and disconnecting the MUT-II/III. Connect the MUT-II/III to the diagnosis connector (16- pin). Turn the ignition switch to the ON position. Read a diagnosis code to refer to that the SRS is operating properly except an open in the seat belt with pre-tensioner circuit. Turn the ignition switch to "LOCK" (OFF) position. DANGER Wait at least 60 seconds after the disconnection of the battery cable before any further job (Refer to ). Disconnect the negative battery cable and insulate with tape.
| >>B<< PRE-TENSIONER CONNECTOR CONNECTION Connect the pretensioner connector then securely lock the locking button of the harness-side connector.
| >> C<< POST-INSTALLATION INSPECTION Connect the negative battery cable. Turn the ignition key to "ON" position.
| Does the SRS warning lamp illuminate for about 7 seconds, and then remain extinguished for at least 5 seconds after turning OFF? If no, refer to troubleshooting (Refer to).

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SEAT BELTS WITH PRE-TENSIONER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation