[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

DATA LIST REFERENCE TABLE
Item No. | Check item | Check condition | Normal condition
--- | --- | --- | ---
01 | Auto-cruise control switch | MAIN | MAIN switch: ON | ON
MAIN switch: OFF | OFF
02 | SET/COAST | MAIN switch: ON | SET switch: ON | ON
SET switch: OFF | OFF
03 | RESUME/ACCELERATING | RESUME switch: ON | ON
RESUME switch: OFF | OFF
04 | CANCEL | CANCEL switch: ON | ON
CANCEL switch: OFF | OFF
05 | Stop lamp switch (for stop lamp circuit) | Brake pedal: Depressed | ON
Brake pedal: Released | OFF
06 | Stop lamp switch (for auto-cruise control circuit) | Brake pedal: Depressed | ON
Brake pedal: Released | OFF
07 | Inhibitor switch | Selector lever: N or P position | ON
Selector lever: Other than N or P position | OFF
08 | Accelerator switch (Idle switch) | Accelerator pedal: Depressed | OFF
Accelerator pedal: Released | ON
09 | Auto-cruise control operation | Auto-cruise control: active | ON
Auto-cruise control: Inactive | OFF
10 | Vehicle speed signal | Road test the vehicle | The speedometer and MUT-II/III display the same value.
11 | Throttle position sensor (main) | Remove the intake air hose at the throttle body Disconnect the throttle position sensor, and then connect terminal numbers No. 3, No. 4, No. 5 and No. 6 with the use of the special tool: MB991658. Ignition switch: ON | Fully close the throttle valve with your finger | 300 - 700 mV
Fully open the throttle valve with your finger | 4,000 mV or more
No load | 500 - 700 mV
Shift lever: "N" → "D" | The voltage rises
12 | Accelerator pedal position sensor (main) | Ignition switch: ON | Release the accelerator pedal | 800 - 1,000 mV <R.H. drive vehicles> 350 - 950 mV <L.H. drive vehicles>
Depress the accelerator pedal gradually | Increases in response to the pedal depression stroke
Depress the accelerator pedal fully | 4,000 mV or more
13 | Cancel code | Ignition switch: "ON" | The cancel code, which set when the auto-cruise control system was cancelled at the last time, is set again.

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation