[14] ENGINE COOLING - - ON-VEHICLE SERVICE - ENGINE COOLANT LEAK CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

ON-VEHICLE SERVICE

| ENGINE COOLANT LEAK CHECK WARNING When pressure testing the cooling system, slowly release cooling system pressure to avoid getting burned by hot coolant. CAUTION Be sure to completely clean away any moisture from the places checked. When the tester is taken out, be careful not to spill any coolant. Be careful when installing and removing the tester and when testing not to deform the filler neck of the radiator.
| Check that the coolant level is up to the filler neck. Install a radiator tester and apply 160 kPa pressure, and then check for leakage from the radiator hose or connections. If there is leakage, repair or replace the appropriate part.

[14] ENGINE COOLING - - ON-VEHICLE SERVICE - ENGINE COOLANT LEAK CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation