[13D] FUEL SUPPLY - - FUEL TANK - FUEL TANK PUMP AND GAUGE ASSEMBLY DISASSEMBLY AND REASSEMBLY <4WD> | PRINT PAGE / INDEX / PRIOR / NEXT

FUEL TANK PUMP AND GAUGE ASSEMBLY DISASSEMBLY AND REASSEMBLY <4WD>
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Gasket
|  | 2. | Fuel tank gauge unit connector connection
|  | 3. | Fuel tank gauge unit
|  | 4. | Fuel tank pump connector connection
|  | 5. | Fuel pump bracket
|  | 6. | Fuel pump hose
|  | 7. | Fuel tank assist pump <4G63, 4G64>
|  | 8. | Fuel pump tube <4G63, 4G64>
|  | 9. | Fuel pump pressure regulator <4G69>
| >>A<< | 10. | O-ring
|  | 11. | Fuel pump bracket
|  | 12. | Fuel tank pump
|  | 13. | Fuel tank pump cushion
| >>A<< | 14. | Fuel tank grommet
|  | 15. | Fuel tank filter assembly
| REASSEMBLY SERVICE POINT
| >>A<< FUEL TANK GROMMET/O-RING INSTALLATION Apply gasoline on the grommet and the O-ring before mounting them to prevent damage or twisting.

[13D] FUEL SUPPLY - - FUEL TANK - FUEL TANK PUMP AND GAUGE ASSEMBLY DISASSEMBLY AND REASSEMBLY <4WD> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation