[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MB991502 | MUT-II sub-assembly | Check the SWS (The MUT-II displays DTCs and pulse check)
| MB991955 A: MB991824 B: MB991827 C: MB991910 D: MB991911 E: MB991825 F: MB991826 | MUT-III sub-assembly A: Vehicle Communication Interface (V. C. I.) B: MUT-III USB cable C: MUT-III main harness A (Vehicles with CAN communication system) D: MUT-III main harness B (Vehicles without CAN communication system) E: MUT-III measurement adapter F: MUT-III trigger harness | SWS communication line check (ECU check and service data) CAUTION MUT-III main harness B (MB991911) should be used. MUT-III main harness A should not be used for this vehicle.
| MB991862 A: MB991806 B: MB991812 C: MB991822 | SWS monitor kit A: SWS monitor cartridge B: SWS monitor harness (for column-ECU) C: Probe harness | SWS communication line check (ECU check and service data)
| MB991529 | Diagnosis code check harness | Input signal check by using a voltmeter
| MB991223 A: MB991219 B: MB991220 C: MB991221 D: MB991222 | Harness set A: Test harness B: LED harness C: LED harness adapter D: Probe | Continuity check and voltage measurement at harness wire or connector A: For checking connector pin contact pressure B: For checking power supply circuit C: For checking power supply circuit D: For connecting a locally sourced tester
| MB991854 | SWS monitor harness (for 13-pin connector) | SWS communication line check (ECU check and service data)

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation