[52A] INTERIOR - - FRONT SEAT ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

FRONT SEAT ASSEMBLY

REMOVAL AND INSTALLATION
<L.H. DRIVE VEHICLES>
Pre-removal and Post-installation Operation Removal and Installation of Rear Floor Console Assembly (Refer to ).
|  | 1. | Head restraint
|  | 2. | Heated seat switch <Option - Vehicles for Argentina>
|  |  | Front seat assembly removal steps
--- | --- | --- | ---
|  | 3. | Front seat anchor cover
|  | 4. | Seat anchor cover outer
|  | 5. | Seat anchor cover inner
|  | 6. | Heater harness connector <Option - Vehicles for Argentina>
|  | 7. | Seat belt switch connector <GCC (Driver’s side)>
| >>A<< | 8. | Front seat assembly
<R.H. DRIVE VEHICLES> CAUTION For the removal of the front seat assembly on vehicles with the side-air bags, refer to GROUP 52B, Service Precautions and Air Bag Module and Clock Spring .
Pre-removal and Post-installation Operation Removal and Installation of Floor Console Assembly (Refer to ).
|  | 1. | Head restraint
|  |  | Front seat assembly removal steps
--- | --- | --- | ---
|  | 2. | Front seat anchor cover
|  | 3. | Seat anchor cover outer
|  | 4. | Seat anchor cover inner
|  | 5. | Seat belt switch connector <Vehicles for Hong Kong and Australia (Driver’s side)>
|  | 6. | Side-air bag module (squib) connector <Vehicles with side-air bag system>
| >>A<< | 7. | Front seat assembly
| INSTALLATION SERVICE POINT
| >>A<< FRONT SEAT ASSEMBLY INSTALLATION
| Temporarily tighten the nuts and bolts in all mounting locations shown in the illustration with no load applied to the front seat cushion and check the operation of the seat slide. Tighten the nuts and bolts in all mounting locations to the specified torque.

[52A] INTERIOR - - FRONT SEAT ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation