[51] EXTERIOR - - REAR BUMPER ASSEMBLY - REAR BUMPER ASSEMBLY - DISASSEMBLY AND REASSEMBLY <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND REASSEMBLY <2400>
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Side cover
|  | 2. | Muffler cover
|  | 3. | Rear bumper cover
<<A>> | >>A<< | 4. | Rivets
|  | 5. | Rear bumper side plate
|  | 6. | Rear bumper harness
|  | 7. | Rear bumper reinforcement
|  | 8. | Licence plate lamp assembly
|  | 9. | Reflector
|  | 10. | Licence plate bracket
|  | 11. | Rear bumper extension <SPORT GEAR, GLS, XLS>
|  | 12. | Rear bumper face
| DISASSEMBLY SERVICE POINT
| <<A>> RIVETS REMOVAL
| Use a drill (&phis;4.0 mm) to make a hole in the rivet to break it, and then remove the rivet.
| REASSEMBLY SERVICE POINT
| >>A<< RIVETS INSTALLATION
| Use recommended tool shown in the illustration to connect the rivet by the following procedure. Insert the rivet into the base material (rear bumper face, rear bumper side plate). Place the recommended tool over section A of rivet. While pushing the flange surface of the rivet with the recommended tool, press the handle of the tool. The thin part of section A of the rivet will break and the rivet will then be attached.

[51] EXTERIOR - - REAR BUMPER ASSEMBLY - REAR BUMPER ASSEMBLY - DISASSEMBLY AND REASSEMBLY <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation