[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - AUTO-CRUISE CONTROL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

AUTO-CRUISE CONTROL

REMOVAL AND INSTALLATION
<AUTO-CRUISE VACUUM PUMP>
|  |  | Auto-cruise vacuum pump removal steps
--- | --- | --- | ---
|  | 1. | Vacuum hoses
|  | 2. | Vacuum hose clips
|  | 3. | Vacuum pipe
|  | 4. | Auto-cruise vacuum pump connector
|  | 5. | Auto-cruise vacuum pump assembly
|  | 6. | Auto-cruise vacuum pump bracket
|  | 7. | Spacers
|  | 8. | Rubber mounts
|  | 9. | Auto-cruise vacuum pump bracket
<SWITCHES, CONTROL UNIT AND SENSORS> CAUTION Before removing the steering wheel and air bag module assembly and air bag module, refer to GROUP 52B - Air bag module and clock spring . When removing and installing the steering wheel and air bag module assembly, do not let it bump against the air bag module.
|  |  | Auto-cruise control switch removal
--- | --- | --- | ---
|  | • | Auto-cruise control switch (Refer to GROUP 52B, Air Bag Module(s) and Clock Spring )
|  |  | Auto-cruise control-ECU removal steps
|  | • | Centre lower panel and centre lower box <L.H. drive vehicles> (Refer to GROUP 52A - Instrument panel )
|  | 10. | Auto-cruise control-ECU
|  | 11. | Auto-cruise control-ECU bracket <R.H. drive vehicles>
|  |  | Sensor removal
|  | • | Inhibitor switch (Refer to GROUP 23B, Transmission )
|  | • | Throttle body assembly (Refer to GROUP 13B, Throttle body assembly )
|  | • | Stop lamp switch (Refer to GROUP 35A, Brake pedal )

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - AUTO-CRUISE CONTROL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation