[54A] CHASSIS ELECTRICAL - - HEADLAMP - ON-VEHICLE SERVICE - LUMINOUS INTENSITY MEASUREMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| LUMINOUS INTENSITY MEASUREMENT Set the headlamps to high-beam. Using a photometer, and following its manufacturer's instruction manual, measure the headlamp centre intensity and check to be sure that the limit value is satisfied. Limit: 30,000 cd or more {When a screen is set 25m ahead of the vehicle} NOTE: When measuring the intensity, maintain an engine speed of 2,000 r/min., with the battery fully charged. There may be special local regulations pertaining to headlamp intensity. Be sure to make any adjustments necessary to satisfy such regulations. If an illuminometer is used to make the measurements, convert its values to photometer values by using the following formula. I =E x r2 : I = Intensity (cd) E = Illumination (lux) r = Distance (m) from headlamps to illuminometer

[54A] CHASSIS ELECTRICAL - - HEADLAMP - ON-VEHICLE SERVICE - LUMINOUS INTENSITY MEASUREMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation