[11F] ENGINE OVERHAUL <4G69> - - TORQUE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

TORQUE SPECIFICATIONS
Item | N·m
--- | ---
Alternator and ignition system
Auto-tensioner bracket bolt M10 | 44 ± 10 N·m
Auto-tensioner bracket bolt M8 | 22 ± 4 N·m
Camshaft position sensing cylinder bolt | 22 ± 4 N·m
Camshaft position sensor bolt | 8.5 ± 0.5 N·m
Camshaft position sensor support bolt | 14 ± 1 N·m
Connector bracket bolt | 10 ± 1 N·m
Crankshaft pulley bolt | 25 ± 4 N·m
Alternator bolt | 49 ± 9 N·m
Alternator pivot nut | 44 ± 10 N·m
Idler pulley bolt | 79 ± 5 N·m
Ignition coil bolt | 10 ± 2 N·m
Oil level gauge guide bolt | 13 ± 1 N·m
Spark plugs | 25 ± 5 N·m
Water pump pulley bolt | 8.8 ± 1 N·m
Exhaust manifold
Oxygen sensor | 49 ± 5 N·m
Engine hanger bolt | 24 ± 3 N·m
Exhaust manifold cover bolt | 14 ± 1 N·m
Exhaust manifold bracket B bolt | 34 ± 5 N·m
Exhaust manifold nut | 49 ± 5 N·m
Exhaust manifold bracket A bolt | 36 ± 5 N·m
Timing belt
Auto-tensioner bolt | 24 ± 2 N·m
Camshaft sprocket bolt | 89 ± 9 N·m
Counterbalance shaft sprocket bolt | 45 ± 3 N·m
Crankshaft bolt | 167 N·m
Crankshaft angle sensor bolt | 11 ± 1 N·m
Engine support bracket bolt | 49 ± 5 N·m
Generator bracket bolt | 49 ± 9 N·m
Idler pulley bolt | 35 ± 6 N·m
Oil pump sprocket nut | 54 ± 4 N·m
Tensioner "B" bolt | 19 ± 3 N·m
Tensioner arm bolt | 21 ± 4 N·m
Tensioner pulley bolt | 49 ± 4 N·m
Timing belt cover bolt M6 (Bolt, washer assembly) | 9.0 ± 1.0 N·m
Timing belt cover bolt M6 (Flange bolt and nut) | 11 ± 1 N·m
Timing belt cover bolt M8 | 14 ± 1 N·m
Fuel and emission parts
EGR valve bolt | 24 ± 3 N·m
Injectors and delivery pipe bolt | 11 ± 1 N·m
Solenoid valve bracket bolt | 11 ± 1 N·m
Solenoid valve nut | 9.0 ± 1.0 N·m
Throttle body bolt | 18 ± 3 N·m
Vacuum pipe and hose bolt | 11 ± 1 N·m
Intake manifold and water pump
Manifold differential pressure sensor bolt | 5.0 ± 1.0 N·m
Engine coolant temperature gauge unit | 11 ± 1 N·m
Engine coolant temperature sensor | 30 ± 9 N·m
Engine hanger bolt | 24 ± 3 N·m
Harness bracket bolt | 11 ± 1 N·m
Intake manifold bolt | 24 ± 3 N·m
Intake manifold nut | 20 ± 2 N·m
Intake manifold stay bolt | 31 ± 3 N·m
Detonation sensor | 23 ± 2 N·m
Oil pressure switch | 19 ± 3 N·m
Thermostat housing bolt | 24 ± 4 N·m
Water inlet fitting bolt | 13 ± 2 N·m
Water inlet pipe bolt | 13 ± 2 N·m
Water outlet fitting bolt | 13 ± 2 N·m
Water pump bolt | 14 ± 1 N·m
Rocker arms and camshaft
Accumulator body bolt | 44 ± 5 N·m
Oil control valve bolt | 11 ± 1 N·m
PCV valve | 10 ± 2 N·m
Rocker arms and rocker arm shaft bolt <exhaust side> | 13 ± 1 N·m
Rocker arms and rocker arm shaft bolt <intake side> | 31 ± 3 N·m
Rocker cover bolt | 3.5 ± 0.5 N·m
Taper plug | 47 ± 7 N·m
Cylinder head and valves
Cylinder head bolt | 78 ± 2 N·m → 0 N·m → 20 ± 1 N·m →+90°→+90°
Oil pan and oil pump
Drain plug | 39 ± 5 N·m
Flange bolt | 36 ± 3 N·m
Front case bolt | 23 ± 3 N·m
Oil filter bracket bolt | 19 ± 3 N·m
Oil filter other than MITSUBISHI genuine filter | 17 ± 3 N·m
Oil filter part number MD356000 | 14 ± 2 N·m
Oil pan bolt | 9.0 ± 3.0 N·m
Oil pump cover bolt | 17 ± 1 N·m
Oil pump cover screw | 10 ± 2 N·m
Oil screen bolt | 19 ± 3 N·m
Plug | 23 ± 3 N·m
Relief plug | 44 ± 5 N·m
Transmission stay bolt | 22 ± 4 N·m
Piston and connecting rod
Connecting rod cap nut | 20 ± 2 N·m →+90° to 94°
Crankshaft and cylinder block
Bearing cap bolt | 25 ± 2 N·m →+90°
Bell housing cover bolt | 9.0 ± 1.0 N·m
Drive plate bolt | 132 ± 5 N·m
Oil seal case bolt | 11 ± 1 N·m
Rear plate bolt | 11 ± 1 N·m

[11F] ENGINE OVERHAUL <4G69> - - TORQUE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation