[15] INTAKE AND EXHAUST - - AIR INTAKE SYSTEM - INTAKE MANIFOLD | PRINT PAGE / INDEX / PRIOR / NEXT

INTAKE MANIFOLD
<4G6-Non-Turbo> In terms of basic structure, the intake manifold are the same as the 4G6 engine intake manifold used in the SPACE RUNNER and SPACE WAGON.
<4G6-Turbo> The aluminum inlet manifold equipped with the EGR passage is adopted.
<4G69> The intake manifold is designed to improve the low, middle and high torque by optimizing the port diameter and length. A port opening with an optimized bell mouth shape and improved the inside roughness of the port reduces airflow resistance.

[15] INTAKE AND EXHAUST - - AIR INTAKE SYSTEM - INTAKE MANIFOLD | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation