[11D] ENGINE OVERHAUL <4G6-DOHC> - - REWOK DIMENSIONS | PRINT PAGE / INDEX / PRIOR / NEXT

REWOK DIMENSIONS
Item | Standard value
--- | ---
CYLINDER HEAD AND VALVES
Diameter of oversize valve seat ring hole in cylinder head mm | Intake | 0.3 oversize | 35.30 - 35.33
0.6 oversize | 35.60 - 35.63
Exhaust | 0.3 oversize | 33.30 - 33.33
0.6 oversize | 33.60 - 33.63
Diameter of oversize valve guide hole in cylinder head mm | 0.05 oversize | 12.05 - 12.07
0.25 oversize | 12.25 - 12.27
0.50 oversize | 12.50 - 12.52

[11D] ENGINE OVERHAUL <4G6-DOHC> - - REWOK DIMENSIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation