[51] EXTERIOR - - MOULDINGS - MOULDINGS - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

MOULDINGS

REMOVAL AND INSTALLATION
|  |  | Roof drip moulding removal steps <Vehicles without roof rail>
--- | --- | --- | ---
<<A>> | >>A<< | 1. | Roof drip moulding
|  |  | Roof drip moulding removal steps <Vehicles with roof rail>
|  | • | Roof rail (Refer to <2000> or <2400> ).
<<A>> | >>A<< | 2. | Front roof drip moulding
<<A>> | >>A<< | 3. | Centre roof drip moulding
| REMOVAL SERVICE POINT
| <<A>> ROOF DRIP MOULDING REMOVAL CAUTION If the moulding has become warped, it should not be reused.
| Use special tool: window moulding remover MB990449 to pry out the moulding.
| INSTALLATION SERVICE POINT
| >>A<< ROOF DRIP MOULDING INSTALLATION Install the clips to the roof drip moulding before installing the moulding to the vehicle body.

[51] EXTERIOR - - MOULDINGS - MOULDINGS - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation