[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ON-VEHICLE SERVICE - ACCELERATOR CABLE CHECK AND ADJUSTMENT <4G69-L.H. DRIVE VEHICLES> | PRINT PAGE / INDEX / PRIOR / NEXT

| ACCELERATOR CABLE CHECK AND ADJUSTMENT <4G69-L.H. DRIVE VEHICLES> Turn A/C and lights OFF. Inspect and adjust at no load. Warm engine until stabilized at idle. Confirm idle speed is at standard value. Standard value: 750 ± 100 r/min Stop engine. [ignition switch: LOCK (OFF) position]. Confirm there are no sharp bends in the accelerator cable. Check the inner cable for correct slack. Standard value: 1.0 - 2.0 mm
| If there is too much slack or no slack, adjust play by the following procedures. Loosen the lock nut and adjusting nut to release the cable. Tighten the adjusting nut until the inner cable play is at the standard value, and then tighten the lock nut.

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ON-VEHICLE SERVICE - ACCELERATOR CABLE CHECK AND ADJUSTMENT <4G69-L.H. DRIVE VEHICLES> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation