[14] ENGINE COOLING - - WATER PUMP - REMOVAL AND INSTALLATION <4G63-SOHC, 4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

WATER PUMP

REMOVAL AND INSTALLATION <4G63-SOHC, 4G64-SOHC>
Pre-removal and Post-installation Operation Engine Coolant Draining and Supplying (Refer to ). Timing Belt Removal and Installation (Refer to GROUP 11A, Timing Belt ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Alternator brace
|  | 2. | Water pump
|  | 3. | Water pump gasket
| >>A<< | 4. | O-ring
| INSTALLATION SERVICE POINT
| >>A<< O-RING INSTALLATION
| Fit the O-ring to the groove in the water inlet pipe. Then lubricate the O-ring and the inside of the water pump with water, and then insert the pipe to the water pump.

[14] ENGINE COOLING - - WATER PUMP - REMOVAL AND INSTALLATION <4G63-SOHC, 4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation