[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - CHECK AT IMMOBILIZER-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

CHECK AT IMMOBILIZER-ECU
TERMINAL VOLTAGE CHECK
Terminal No. | Signal | Inspection condition | Terminal voltage
--- | --- | --- | ---
1 | Immobilizer-ECU power supply | Ignition switch: "LOCK" (OFF) | 0V
Ignition switch: "ON" | Battery positive voltage
2 | - | - | -
3 | Engine-A/T-ECU | - | -
4 | Immobilizer-ECU earth | Always | 0V

[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - CHECK AT IMMOBILIZER-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation