[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - ACCELERATOR PEDAL POSITION SENSOR CHECK <Vehicles except for Australia, South africa and Hong kong > | PRINT PAGE / INDEX / PRIOR / NEXT

| ACCELERATOR PEDAL POSITION SENSOR CHECK <Vehicles except for Australia, South africa and Hong kong >
| Disconnect the accelerator pedal position sensor connector. Measure resistance between terminal No. 2 (main power supply) and No. 1 (main earth) as well as between terminal No. 8 (sub power supply) and terminal No. 7 (sub earth) of the sensor connector. Standard valve: 3.5 - 6.5 kΩ Measure resistance between terminal No. 2 (main power supply) and No. 3 (main output) as well as between terminal No. 8 (sub power supply) and No. 6 (sub output) of the sensor connector.
Normal condition:
Depress the accelerator pedal slowly. | Resistance value changes in accordance with the accelerator pedal depression smoothly.
| If not within the standard value, or resistance value does not change smoothly, replace the accelerator pedal position sensor. NOTE: After replacement, adjust the accelerator pedal position sensor. (Refer to .)

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - ACCELERATOR PEDAL POSITION SENSOR CHECK <Vehicles except for Australia, South africa and Hong kong > | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation