[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - G-SENSOR <4WD> - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| G-SENSOR CHECK
| Disconnect the G-sensor connector and connect special tool Test Harness Set (MB991348), between terminals of the disconnected connector. With the ignition switch turned to the "ON" position, read the voltage between terminals number 2 and number 3. Standard Value: 2.4 - 2.6 V With special tool Test Harness Set (MB991348) connected, rotate so that the arrow faces straight down. Read output voltage between terminals number 2 and number 3. Standard Value: 1.0 - 4.0 V If the voltage deviates from the standard value, make sure that nothing is wrong with the power supply wire and earth wire and then replace the G-sensor.

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - G-SENSOR <4WD> - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation