[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM PROCEDURES - Inspection Procedure 5: Accelerator Pedal Operation is not Smooth (Over Acceleration) <4G69-R.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection Procedure 5: Accelerator Pedal Operation is not Smooth (Over Acceleration) <4G69-R.H. drive vehicles>
DIAGNOSIS PROCEDURE
STEP 1. Check if the accelerator pedal and the accelerator pedal are installed correctly. Q: Are the accelerator pedal and the accelerator pedal installed correctly? YES: Go to Step 2. NO: Replace and reinstall the accelerator pedal (Refer to ). Go to Step 3.
STEP 2. Check the MUT-II/III diagnosis code Q: Is any diagnosis code set? YES: Refer to GROUP 13C, Troubleshooting - Inspection Chart for Diagnosis Code . NO: Go to Step 3.
STEP 3. Retest the system. Q: Does the accelerator pedal work normally? YES: The procedure is complete. NO: Return to Step 1.

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM PROCEDURES - Inspection Procedure 5: Accelerator Pedal Operation is not Smooth (Over Acceleration) <4G69-R.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation