[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - SYMPTOM PROCEDURES - Inspection Procedure 2: When the Selector Lever is Moved to "N" Range, Auto-cruise Control is not Cancelled. | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection Procedure 2: When the Selector Lever is Moved to "N" Range, Auto-cruise Control is not Cancelled.
COMMENTS ON TROUBLE SYMPTOM The inhibitor switch circuit is suspected.
PROBABLE CAUSES Malfunction of the inhibitor switch. Malfunction of the connector. Malfunction of the harness. Malfunction of the engine-A/T-ECU.
DIAGNOSIS Refer to GROUP 23A, Symptom Procedures - Inspection Procedure 16: Inhibitor switch system <4G69> .

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - SYMPTOM PROCEDURES - Inspection Procedure 2: When the Selector Lever is Moved to "N" Range, Auto-cruise Control is not Cancelled. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation