[54A] CHASSIS ELECTRICAL - - SPEED ALARM <Vehicles for GCC> - CHECK AT SPEED ALARM-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

CHECK AT SPEED ALARM-ECU
TERMINAL VOLTAGE CHECK
Terminal No. | Signal | Inspection condition | Terminal voltage
--- | --- | --- | ---
1 | Speed alarm-ECU power supply | Ignition switch: "LOCK" (OFF) | 0 V
Ignition switch: "ON" | Battery positive voltage
2 - 3 | - | - | -
4 | Engine-A/T-ECU | - | -
5 - 7 | - | - | -
8 | Speed alarm-ECU earth | Always | 0 V

[54A] CHASSIS ELECTRICAL - - SPEED ALARM <Vehicles for GCC> - CHECK AT SPEED ALARM-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation