[51] EXTERIOR - - REAR BUMPER ASSEMBLY - REAR BUMPER ASSEMBLY - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <2400>
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Rear combination lamp
|  | • | Rear end trim
|  | 1. | Mud guard <Except Hong Kong>
|  | 2. | Rear splash shield
|  | 3. | Tapping screw
|  | • | Ventilation cap (Refer to GROUP 52A, Trims ).
<<A>> |  | 4. | Clips
|  | • | Rear bumper harness connector connection
|  | 5. | Rear bumper assembly
| REMOVAL SERVICE POINT
| <<A>> CLIPS REMOVAL
| Remove the clip with a pair of pliers by removing the claw of the clip from the cabin side.

[51] EXTERIOR - - REAR BUMPER ASSEMBLY - REAR BUMPER ASSEMBLY - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation