[54A] CHASSIS ELECTRICAL - - REAR FOG LAMP <2400 for Hong Kong spec. and Argentina> - REAR FOG LAMP - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

REAR FOG LAMP

REMOVAL AND INSTALLATION
|  |  | Rear fog lamp switch removal steps
--- | --- | --- | ---
|  | 1. | Instrument panel driver’s side garnish (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 2. | Meter bezel (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 3. | Fog lamp switch bracket
|  | 4. | Fog lamp switch (front fog lamp switch and rear fog lamp switch)
|  |  | Rear fog lamp removal steps
|  | • | Rear bumper (Refer to GROUP 51, Rear bumper ).
|  | 5. | Rear fog lamp assembly
|  | 6. | Rear fog lamp body and lens
|  | 7. | Socket
|  | 8. | Bulb

[54A] CHASSIS ELECTRICAL - - REAR FOG LAMP <2400 for Hong Kong spec. and Argentina> - REAR FOG LAMP - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation