[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

DATA LIST REFERENCE TABLE
Item No. | Check item | Check condition | Normal condition
--- | --- | --- | ---
01 | Auto-cruise control switch | MAIN | MAIN switch: ON | ON
MAIN switch: OFF | OFF
02 | SET/COAST | MAIN switch: ON | SET switch: ON | ON
SET switch: OFF | OFF
03 | RESUME/ACCELERATING | RESUME switch: ON | ON
RESUME switch: OFF | OFF
04 | CANCEL | CANCEL switch: ON | ON
CANCEL switch: OFF | OFF
05 | Stop lamp switch (for stop lamp circuit) | Brake pedal: Depressed | ON
Brake pedal: Released | OFF
08 | Accelerator switch (Idle switch) | Accelerator pedal: Depressed | OFF
Accelerator pedal: Released | ON
10 | Vehicle speed signal | Road test the vehicle | The speedometer and MUT-II/III display the same value.
13 | Throttle position sensor (TPS) | Ignition switch: ON | Accelerator pedal: Released | 535 - 735 mV
Accelerator pedal: Depressed | Increased according to accelerator pedal stroke.
Accelerator pedal: Fully depressed | 4,500 - 5,000 mV
14 | Inhibitor switch | Selector lever: N or P position | ON
Selector lever: Other than N or P position | OFF
15 | Over drive detective (OD-OFF→OD-ON signal) | Driving on level road (No OD-OFF request) | OFF
Driving on uphill road (OD-OFF request) | ON

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation