[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

| DIAGNOSIS FUNCTION
| READING DIAGNOSIS CODES
| WHEN USING THE MUT-II/III Refer to GROUP 00, How to Use Troubleshooting/Inspection Service Points .
| WHEN USING THE ABS WARNING LAMP Turn the ignition switch to the "LOCK" (OFF) position.
| Use special tool diagnosis code check harness (MB991529) to earth number 1 terminal (diagnosis control terminal) of the diagnosis connector. Turn the ignition switch to the "ON" position.
| Read out a diagnosis code by observing how the warning lamp flashes.
When the diagnosis code No. 24 is output | When no diagnosis code is output
--- | ---
| Turn the ignition switch to the "LOCK" (OFF) position. Disconnect special tool diagnosis code check harness (MB991529).
| ERSING DIAGNOSIS CODES
| WHEN USING THE MUT-II/III Refer to GROUP 00, How to Use Troubleshooting/Inspection Service Points .
| WHEN NOT USING THE MUT-II/III NOTE: If the ABS-ECU functions have stopped due to the fail-safe function, the diagnosis code cannot be erased. Turn the ignition switch to the "LOCK" (OFF) position.
| Use special tool diagnosis code check harness (MB991529) to earth number 1 terminal of the diagnosis connector.
| Depress the brake pedal and hold it. Turn the ignition switch to the "ON" position. After turning the ignition switch to the "ON", release the pedal within three seconds. Repeat this process of pressing and releasing the brake pedal 10 continuous times. Turn the ignition switch to the "LOCK" (OFF) position. Disconnect special tool diagnosis code check harness (MB991529).

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation