[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - PURGE CONTROL SOLENOID VALVE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| PURGE CONTROL SOLENOID VALVE CHECK NOTE: When disconnecting the vacuum hose, always make a mark so that it can be reconnected at original position.
| Disconnect the vacuum hose from the solenoid valve. Disconnect the harness connector. Connect a hand vacuum pump to nipple (A) of the solenoid valve (refer to the illustration at left). Check airtightness by applying a vacuum with voltage applied directly from the battery to the purge control solenoid valve and without applying voltage.
Battery voltage | Normal condition
--- | ---
Applied | Vacuum leaks
Not applied | Vacuum maintained
Measure the resistance between the terminals of the solenoid valve. Standard value: 30 - 34 Ω (at 20°C) <4G63, 4G69 Except for Brazil and Chile> 22 - 26 Ω (at 20°C) <4G69, Vehicles for Brazil and Chile>

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - PURGE CONTROL SOLENOID VALVE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation