[11A] ENGINE MECHANICAL <4G6-SOHC> - - CRANKSHAFT OIL SEAL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

CRANKSHAFT OIL SEAL

REMOVAL AND INSTALLATION
|  |  | Crankshaft front oil seal removal steps
--- | --- | --- | ---
|  | • | Valve timing belt, balancer timing belt (Refer to ).
| >>D<< | 1. | Crankshaft balancer shaft drive sprocket
|  | 2. | Crankshaft key
| >>C<< | 3. | Crankshaft front oil seal
|  |  | Crankshaft rear oil seal removal steps
|  | • | Transmission assembly [Refer to GROUP 23A, Transmission Assembly <4G63> , Refer to GROUP 23A, Transmission Assembly <4G64> ].
<<A>> | >>B<< | 4. | A/T drive plate bolts
|  | 5. | A/T drive plate adapter plate
|  | 6. | A/T drive plate <4G63>
|  | 7. | A/T drive plate <4G64>
|  | 8. | Crankshaft bush
| >>A<< | 9. | Crankshaft rear oil seal
| REMOVAL SERVICE POINT
| <<A>>A/T DRIVE PLATE BOLTS REMOVAL
| Use special tool flywheel stopper (MD998781) to secure the A/T drive plate. Remove the A/T drive plate bolts.
| INSTALLATION SERVICE POINTS
| >>A<< CRANKSHAFT REAR OIL SEAL INSTALLATION
| Apply a small amount of engine oil to the entire inner diameter of the oil seal lip. Use the following special tools to press-fit the oil seal. Installer bar (MB990938) Crankshaft rear oil seal installer (MD998776)
| >>B<<A/T DRIVE PLATE BOLTS INSTALLATION
| Use special tool flywheel stopper (MD998781) to secure the A/T drive plate in the same manner as removal. Tighten the A/T drive plate bolts to the specified torque. Tightening torque: 132 ± 5 N·m
| >>C<< CRANKSHAFT FRONT OIL SEAL INSTALLATION
| Apply a small amount of engine oil to the entire inner diameter of the oil seal lip. Apply a small amount of engine oil to the outer diameter of special tool crankshaft front oil seal guide (MD998285) and install it to the crankshaft. Use special tool crankshaft front oil seal installer (MD998375) to press-fit the oil seal.
| >>D<< CRANKSHAFT BALANCER SHAFT DRIVE SPROCKET INSTALLATION
| Clean or degrease the front case, the crankshaft and the crankshaft balancer shaft drive sprocket as shown. NOTE: Also clean the degreased surfaces. Install the crankshaft balancer shaft drive sprocket in the direction shown in the illustration.

[11A] ENGINE MECHANICAL <4G6-SOHC> - - CRANKSHAFT OIL SEAL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation