[11C] ENGINE MECHANICAL <4G6-DOHC> - - ON-VEHICLE SERVICE - DRIVE BELT TENSION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

ON-VEHICLE SERVICE

| DRIVE BELT TENSION CHECK CAUTION Check the drive belt tension after turning the crankshaft clockwise one turn or more.
| Make sure that the indicator mark is within the area marked with A in the illustration. If the mark is out of the area, replace the drive belt. (Refer to ). NOTE: The drive belt tension check is not necessary as auto-tensioner is adopted.

[11C] ENGINE MECHANICAL <4G6-DOHC> - - ON-VEHICLE SERVICE - DRIVE BELT TENSION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation