[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - LINE PRESSURE ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| LINE PRESSURE ADJUSTMENT Drain the transmission fluid. NOTE: The hydraulic pressure test must be performed before attempting any adjustments. Remove the valve body cover.
| Turn the adjusting screw shown in the illustration to adjust the line pressure to the standard value. The pressure increases when the screw is turned anti-clockwise. NOTE: When adjusting the line pressure, adjust to the middle of the standard value range. Standard value: 1.01 - 1.05 MPa (Change in pressure for a single full of the adjusting screw: 0.035 MPa) Install the valve body cover, and then pour in the specified amount of A/T fluid. Repeat the hydraulic pressure test. (Refer to .) Readjust the line pressure if necessary.

[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - LINE PRESSURE ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation