[42] BODY - - HOOD - HOOD - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| HOOD SWITCH CONTINUITY CHECK <VEHICLES FOR HONG KONG SPEC>
SWITCH POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
Release (ON) | 1 - 2 | Less than 2 ohms
Depressed (OFF) | 1 - 2 | Open circuit

[42] BODY - - HOOD - HOOD - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation