[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 15: Distortion on AM or on Both AM and FM. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 15: Distortion on AM or on Both AM and FM.
DIAGNOSIS PROCEDURE
STEP 1. Check the degree in which distortion is generated. Q: How much distortion is generated? Occasional distortion: Go to Step 2. Constant distortion: Go to Step 3.
STEP 2. Check by the transmission antenna. Q: Is there distortion by the transmission antenna? YES: The input from the antenna is too big. NO: Go to Step 3.
STEP 3. Check how the speakers are setup. Q: Are any cords coming in contact with the paper cones of the speakers? YES: Move the cords so that they do not come in contact with the paper cones of the speaker. Check that a distortion is resolved. NO: Go to Step 4.
STEP 4. Check the speakers. Remove the speakers. Check to see if there is any ripping of the paper cones or any foreign obstacles in the paper cone. Q: Are the speakers normal? YES: Go to Step 5. NO: Repair or replace the speakers. Check that a distortion is resolved.
STEP 5. Check how the speakers are setup. Q: Check to see if the speakers are setup in a deformed manner. YES: Correct the way the speakers are setup so they are securely setup. Check that a distortion is resolved. NO: Repair or replace the radio and tape or CD player. Check that a distortion is resolved.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 15: Distortion on AM or on Both AM and FM. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation