[11F] ENGINE OVERHAUL <4G69> - - ROCKER ARMS AND CAMSHAFT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| CAMSHAFT
| Measure the cam height. If it is below the limit, replace the camshaft.
| Standard value | Minimum limit
--- | --- | ---
A: Intake low speed cam A | 37.47 mm | 36.97 mm
B: Intake low speed cam B | 37.47 mm | 36.97 mm
C: Intake high speed cam | 37.21 mm | 36.71 mm
D: Exhaust cam | 37.86 mm | 37.36 mm

[11F] ENGINE OVERHAUL <4G69> - - ROCKER ARMS AND CAMSHAFT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation