[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - INTERIOR <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

INTERIOR <2400>
No. | Standard measurement point | Hole shape | Size mm
--- | --- | --- | ---
36 | Front pillar positioning notch (upper) | - | -
37 | Front pillar positioning notch (lower) | - | -
38 | Side roof rail positioning notch (front) | - | -
39 | Side sill positioning notch (front) | - | -
40 | Centre pillar positioning notch (upper) | - | -
41 | Centre pillar positioning notch (lower) | - | -
42 | Side roof rail positioning notch (rear) | - | -
43 | Side sill positioning notch (rear) | - | -
44 | Quarter panel positioning notch (upper) | - | -
45 | Quarter panel positioning notch (lower) | - | -
55 | Centre of floor console mounting hole | Round | 12
56 | Centre of floor carpet mounting hole (Body centre point) | Round | 6
No. | Standard measurement point | Hole shape | Size mm
--- | --- | --- | ---
57 | Centre of rear floor crossmember positioning hole (Body centre point) | Round | 16
58 | Centre of rear shock absorber mounting hole | Round | 12
59 | Centre of rear end trim mounting hole | Round | 8.5
60 | Tip of instrument panel bracket centre (Body centre point) | - | -
61 | Centre of deck crossmember mounting hole (left-upper) | Round | 11
62 | Centre of deck crossmember mounting hole (right-upper) | Round | 11
63 | Centre of deck crossmember mounting hole (left-lower) | Round | 11
64 | Centre of deck crossmember mounting hole (right-lower) | Round | 11
65 | Centre of deck crossmember mounting hole (upper) | Round | 11
66 | Centre of deck crossmember mounting hole (lower) | Round | 11

[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - INTERIOR <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation