[35A] BASIC BRAKE SYSTEM - - ON-VEHICLE SERVICE - BRAKE FLUID LEVEL SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| BRAKE FLUID LEVEL SENSOR CHECK
| The brake fluid level sensor is in good condition if there is no continuity when the float surface is above "MIN" and if there is continuity when the float surface is below "MIN".

[35A] BASIC BRAKE SYSTEM - - ON-VEHICLE SERVICE - BRAKE FLUID LEVEL SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation