[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 25. CLUTCH OPERATION | PRINT PAGE / INDEX / PRIOR / NEXT

| 25. CLUTCH OPERATION
| Check the clutch operation in all driving ranges. Turn up the carpet, etc under the clutch pedal. Check the pedal-to-toeboard clearance when the clutch is just disengaged. Clearance to toeboard when clutch disengaged: Standard value: 105 mm or more
| Verify correct clutch pedal free play. NOTE: For inspection and adjustment of the free play of the clutch pedal, refer to GROUP 2, Periodic Inspection and Maintenance.

[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 25. CLUTCH OPERATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation