[11F] ENGINE OVERHAUL <4G69> - - GENERAL SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL SPECIFICATIONS
Item | Specification
--- | ---
Type | In-line OHV, SOHC
Number of cylinders | 4
Combustion chamber | Pent roof type
Total displacement mL | 2,378
Cylinder bore mm | 87
Piston stroke mm | 100
Compression ratio | 9.5
Valve timing | Intake valve | Opens (BTDC) | 6° <Low speed cam A>
6° <Low speed cam B>
20° <High speed cam>
Closes (ABDC) | 38° <Low speed cam A>
38° <Low speed cam B>
72° <High speed cam>
Exhaust valve | Opens (BBDC) | 60°
Closes (ATDC) | 16°
Lubrication system | Pressure feed, full-flow filtration
Oil pump type | Involute gear type

[11F] ENGINE OVERHAUL <4G69> - - GENERAL SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation