[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - MULTIMODE KEYLESS ENTRY FUNCTION CHECK <VEHICLES FOR HONG KONG SPEC> | PRINT PAGE / INDEX / PRIOR / NEXT

| MULTIMODE KEYLESS ENTRY FUNCTION CHECK <VEHICLES FOR HONG KONG SPEC> Operate the transmitter to check that the power windows, the electric-folding door mirrors and the sunroof work. If they do not work, carry out troubleshooting. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting . NOTE: The adjustment function allows you to change the power window setting from "automatic close (initial setting)" to "automatic open and close" or "without function". Prior to that check, confirm which setting is activated. Prior to that check, confirm whether the electric-folding door mirrors is set to "keyless-linked" or not. The adjustment function allows you to change the sunroof setting from "automatic close (initial setting)" to "without function". Prior to that check, confirm which setting is activated.

[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - MULTIMODE KEYLESS ENTRY FUNCTION CHECK <VEHICLES FOR HONG KONG SPEC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation