[33] FRONT SUSPENSION - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Toe-in | At the centre of tyre tread mm | 1 ± 2
Toe-angle (per wheel) | 0°03' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Steering angle | Inner wheel | 2000 | 34°20' ± 1°30'
2400 | 34°50' ± 1°30'
Outer wheel (reference) | 2000 | 29°10'
2400 | 29°20'
Camber | 2000-SOHC | -0°05' ± 30'*
2000-DOHC | -0°15' ± 30'*
2400 | 0°00' ± 30'*
Caster | 2000-SOHC | 3°30' ± 30'*
2000-DOHC | 3°35' ± 30'*
2400 | 3°10' ± 30'*
Kingpin inclination | 2000-SOHC | 12°55' ± 1°30'
2000-DOHC | 13°10' ± 1°30'
2400 | 12°05' ± 1°30'
Side slip mm (per 1m) | 0 ± 3
Lower arm ball joint starting torque N·m | 0 - 3.9
Protruding length of stabilizer link thread part mm | 2000-SOHC | 22 ± 1.5
2000-DOHC and 2400 | 9.4 ± 0.4
Stabilizer link ball joint turning torque N·m | 2000-DOHC and 2400 | 0.5 - 1.5
NOTE: *: difference between right and left wheels must be less than 30'

[33] FRONT SUSPENSION - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation