[15] INTAKE AND EXHAUST - - INLET MANIFOLD - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| Check the following points; replace the part if a problem is found.
| Intake Manifold Check Check for damage or cracking of any part. Clogging of the negative pressure (vacuum) outlet port, or clogging of the exhaust gas recirculation passages. Using a straight edge and feeler gauge, check for distortion of the cylinder head installation surface. Standard value: 0.15 mm or less Limit: 0.20 mm

[15] INTAKE AND EXHAUST - - INLET MANIFOLD - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation