[37] POWER STEERING - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Steering wheel free play mm | With engine running | - | 30
With engine stopped | 10 or less | -
Steering angle | Inside wheel | 2000 | 34°20' ± 1°30' | -
2400 | 34°50' ± 1°30' | -
Outside wheel (reference) | 2000 | 29°10' | -
2400 | 29°20' | -
Tie rod end ball joint starting torque N·m | 0.5 - 2.5 | -
Tie rod swing resistance N [Tie rod swing torque N·m] | 6 - 19 [1.5 - 4.9] | -
Stationary steering effort N [Fluctuation allowance N] | 29 or less [5.9 or less] | -
Oil pump pressure MPa | Oil pump relief pressure | 8.8 - 9.5 | -
Pressure under no-load conditions | 2000-SOHC | 0.2 - 0.7 | -
2000-DOHC and 2400 | 0.8 - 1.0 | -
Steering gear retention hydraulic pressure | 8.8 - 9.5 | -
Oil pressure switch operating pressure MPa | OFF → ON | 1.5 - 2.0 | -
ON → OFF | 0.7 - 2.0 | -
Steering gear total pinion torque N·m [Change in torque N·m] | 0.7 - 1.6 [0.4 or less] | -
Opening dimension of special tool boot band crimping tool (MB991561) mm | 2.9 | -
Band crimped width mm | 2.4 - 2.8 | -

[37] POWER STEERING - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation